CERES Target Setup

• segmented target

– minimize conversion length to ∼0.3% of X_0 • two radial silicon drift detectors (SDD) – measure vertex and dN_{ch}/dη – provide tracking to RICH – conversion and Dalitz rejection (dE/dx) • W-shield

– absorb slow particles in UV-detector acceptance